

**Audible Beacon Safety Light Instructions**

The Audible Beacon by Ruffwear® is a waterproof, rechargeable LED light that uses audible signals to indicate on/off, low battery, charging, and charge complete. When the light is on, it has a single setting, which offers a bright flashing light. It is comprised of a hard plastic safety light attached to a soft silicone mount that attaches to your harness handle. The silicone mount can be removed to charge the light and to access a clip on the back of the light that can attach the light to backpacks, coats, etc.

**To turn on and off:**

1. Find the soft rubber power button located on one corner of the light.
2. Press and hold the button until you hear an ascending tone sequence.
3. To turn off, press and hold the power button until you hear a descending tone sequence.

**How to attach to your harness handle:**

1. Remove the handle from your harness.
2. With the safety light attached to the silicone mount, slide one side of the handle into the large slot in the silicone mount and up to the metal plate.

**How to remove the light from the silicone mount:**

1. Locate the hard plastic rectangular clip release on one of the light’s sides.
2. Press down on the ridged end of the clip release, while pulling the light away from the silicone mount. Slide the mount off the clip.

**How to charge:**

1. Remove the hard plastic light from the silicone mount. Locate the rectangular rubber cover on the back of the light (next to the clip). Open the cover to access the charging port.
2. Plug the smaller (micro USB) end of the charging cable into the charging port (orient the smooth side of the micro USB towards the clip). The larger end of the cable can be plugged into any USB port.

**Notes:**

1. When you turn on the light (after the ascending tone sequence) there will be a brief pause followed by beeps that audibly represent the pattern of the flashing light (three beeps if the light has a good charge, five beeps if the battery is low).
2. When the light is on, you will hear three reminder beeps every 10 minutes. When battery is low, the beacon will indicate this with 5 beeps every 5 minutes. The light can run up to 12 hours on a charge, and will run about 1 hour in low battery mode). When the battery needs to be recharged, you will hear a rapid repeating beep.
3. When the charging cable is properly connected to both the light and a USB port and is successfully charging, you will hear an ascending tone.
4. The light takes approximately 1.5 hours to fully charge. When it is fully charge, you will hear a slow three tone beep.

Retails for $34.95, available at the GDB store, and via Ruffwear.

YouTube Video <https://youtu.be/eF-Bli3FXI0>